{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["集采材料计划表（一级）"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"集采材料计划表（一级）","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"merged":[[0,0,0,8],[1,0,1,1],[2,0,2,2],[2,3,2,6],[21,0,21,1],[22,4,22,5]],"flags":["formulas_cached_only"]}
["加油站广告材料具体明细及相关要求表"]
["分公司名称：三分公司",null,null,"项目名称：衡永高速房建第一合同段",{"$nulls":3},"项目初步合同金额：4.34亿元"]
["项目类型（自营还是联营）：自营",null,null,"公章上的项目全称：湖南路桥建设集团有限责任公司衡永高速房建第一合同段经理部",{"$nulls":3},"项目详细地点：湖南省衡阳市祁东县衡缘物流园E栋2楼"]
["序号","材料名称","规格型号","单位","预计数量","图样","质量标准及特殊生产工艺要求","推荐供应商","备注"]
[1,"新款品牌柱","12m彩屏品牌柱\n（LED彩屏+数显屏）\n12米新基础","个",4,"=DISPIMG(\"ID_C3476E99715248FA9888944F3D61AAB4\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[2,"转角模组（H1350-1）","高1350，R1000+100\n转角外径R=1000,详见《中国石化综合加能站形象标准手册》。","件",32,"=DISPIMG(\"ID_F021C640FAF74A63BC5331B91A4F3F6F\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[3,"左侧白色底板模组（H1350-2）","高1350，长3780，\n白色底板斜切角度48°，详见《中国石化综合加能站形象标准手册》。","件",24,"=DISPIMG(\"ID_EA963FA2272549759FCE15BEBEAA3A14\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[4,"红色底板模组（H1350-3）","高1350，长2800，详见《中国石化综合加能站形象标准手册》。","件",132,"=DISPIMG(\"ID_917074AFDDE54F8DBCCA5883EA909504\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[5,"调节模组（H1350-4）","高1350，长1400-2800，详见《中国石化综合加能站形象标准手册》。","件",40,"=DISPIMG(\"ID_2F05ED4946214D2F8CF42D4072F241EC\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[6,"右侧白色底板模组（H1350-5）","高1350，长3780\n白色底板斜切角度48°，详见《中国石化综合加能站形象标准手册》。","件",24,"=DISPIMG(\"ID_78BD0939BEC74EFF97A5B706E6811F54\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[7,"朝阳标发光LOGO"," 高1150，详见《中国石化综合加能站形象标准手册》。","件",24,"=DISPIMG(\"ID_2596033CCC364F70AE98A7E8020C407D\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[8,"中文立体发光字","高770，详见《中国石化综合加能站形象标准手册》。","件",24,"=DISPIMG(\"ID_E804F2DFC8504355A774478D17BE33C9\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[9,"英文立体发光字","高490，详见《中国石化综合加能站形象标准手册》。","件",24,"=DISPIMG(\"ID_36C442BA7DBE40D48D2959B49998BE9F\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[10,"H1350(不含帽檐灯带）","高1950，长33150","㎡",272,null,"符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[11,"H1350(不含帽檐灯带）","高1950，长19000","㎡",152,null,"符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[12,"超高檐口上方灰色铝塑板补板","高600，长75150","㎡",184.48,"=DISPIMG(\"ID_786BF03BD8024C8D80AB6143CA1D7B02\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[13,"超高檐口上方灰色铝塑板补板","高600，长93000","㎡",223.2,"=DISPIMG(\"ID_2953A63F0D284D338E0B2E7FE6A73791\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[14,"中石化新款灯箱","3290*1060*645mm详见《中国石化综合加能站形象标准手册》。","个",40,"=DISPIMG(\"ID_A807F70979D740B88F2FC1BE17315595\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[15,"LED防爆灯","150瓦，柴油区15个，汽油区12个","个",108,"=DISPIMG(\"ID_4D34046D7E6D430DA3CBE8B2969D3421\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[16,"进出口指示灯箱","600*850详见《中国石化综合加能站形象标准手册》。","个",8,"=DISPIMG(\"ID_4B232C32A28D4771835D586B6A6D141B\",1)","符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
[17,"布线套管及辅材","布线套管及辅材","项",4,null,"符合中石化油站验收规范中的要求","/","数量为4个加油站的数量"]
["合计",{"$nulls":3},1315.68]
["项目经理：",{"$nulls":3},"总工：",null,null,"编制："]